**Experiment 05 : String Operations Part-I**

**Learning Objective**:

Student should be able to apply string operations (i) Accept

(ii) Display

(iii) Concatenate

(iv) Compare in ALP.

**Tools:** TASM/MASM

**Theory:**

**String Instruction:**

* String is the series of bytes stored sequentially in the memory, string Instructions operate such “Strings”.
* The source elements is taken from the data segment using the SI register.
* The destination element is in the extra segment pointed by the SI register.
* SI and / or DI are incremented/ decremented after each operation depending upon the direction flag “DF” in the flag register.

1. **MOVS: MOVSB/ MOVSW (move string):**

* It is used to transfer a word/ byte from data segment to extra segment.
* The offset of the source in data segment is in SI.
* The offset of the destination in extra segment is in DI.
* SI and DI are incremented / decremented after the transfer depending upon the direction flag.
* Eg: MOVSB ;ES:[DI]🡨 DS:[SI]… byte transfer
  + - * ;SI🡨 SI + OR – 1 … depending upon DF

**;**DI🡨 DI + OR – 1 … depending upon DF

MOVSW ;{ES:[DI], ES:[DI + 1]}🡨 {DS:[SI], DS:[SI + 1]}…word

;SI🡨 SI + or – 2

;DI🡨 DI + or – 2

1. **LODS: LODSB/LODSW (load string)**

* It is used to load AL (or AX) register with a byte (or word) from data segment.
* The offset of the source in data segment is in SI.
* SI is incremented/ decremented after the transfer depending upon the direction flag (DF).
* Eg: LODSB ;AL🡨 DS:[SI]… byte transfer ;SI🡨 SI+ or – 1 … depending upon DF

LODSW;AL🡨 DS:[SI];AH🡨 DS:[SI + 1].. word transfer ;SI🡨 SI + or – 2

1. **STOS: STOSB/ STOSW (store string):**

* It is used to store AL (or AX) into a byte (or word) in the extra segment.
* The offset of the source in extra segment is in DI.
* DI is incremented/ decremented after the transfer depending upon the direction flag

(DF).

* Eg: STOSB ;ES:[DI]🡨 AL… byte transfer ;DI🡨 DI+ or – 1 … depending upon DF

STOSW ;ES:[DI]🡨 AL; ES:[DI + 1]🡨 AH … word transfer ;DI🡨 Di + or – 2 … depending upon DF

1. **CMPS: CMPSB/ CMPSW (compare string):**

* It is used to compare a byte (or word) in the data segment with a byte (or word) in

the extra segment.

* The offset of the byte (or word) in data segment is in SI.
* The offset of the byte (or word) in extra segment is in DI.
* SI and DI are incremented/ decremented after the transfer depending upon the

direction flag.

* Comparison is done by subtracting the byte (or word) from extra segment from the byte (or word) from extra segment. The flag bits are affected, but the result is not stored anywhere.
* Eg: CMPSB ;Compare DS:[SI] with ES:[DI] … byte operation

;SI🡨 SI + or – 1 … depending upon DF

;DI🡨 DI + or – 1 … depending upon DF

CMPSW ;Compare {DS:[SI], DS:[SI + 1]} with {ES:[DI], ES:[DI + 1]}

;SI🡨 SI + or – 2 … depending upon DF

;DI🡨 DI + or – 2 … depending upon DF

1. **SCAS: SCASB/ SCASW (STRING COMPARE ACCUMULATOR)**

* It is used to compare the contents of AL (or AX) with a byte (or word) in the extra segment.
* The offset of the byte (or word) in extra segment is in DI.
* DI is incremented/ decremented after the transfer depending upon the direction flag (DF).
* Comparison is done by subtracting the byte (or word) from extra segment from AL (or AX).
* The flag bits are affected, but the result is not stored anywhere.
* Eg: SCASB ;Compare AL with ES:[DI] … byte operation.

;DI🡨 DI + or – 1 … depending upon DF.

SCASW ;Compare {AX} with {ES:[DI], ES:[DI + 1]} … word operation

;DI🡨 DI + or – 1 … depending upon DF.

**Explanation:**

Using Macro display the Menu for entering string, calculate length, concatenate, compare and exit. Accept the choice from user using INT 21H function 01H.

If choice = 1, call procedure for accepting string. Using interrupt INT 21H, function 0AH accept the string and end procedure. Return back to display Menu.

If choice = 2, call procedure for finding length of the string. Display length and return back to display Menu. (Repeat the process to enter second string)

If choice = 3, call procedure to concatenate two strings. Display the concatenation and return back to display Menu.

If choice = 4, call procedure to compare the two strings. If two strings are equal display, the strings are equal, otherwise display Strings are not equal.

If choice = 5, terminate the program. If any other key is pressed display invalid choice.

**Procedure/Algorithm:**

**Algorithm:**

Step I: Initialize the data and stack memory.

Step II: Using Macro display Menu.

1. Accept 2. Length 3. Concatenate 4. Compare 5. Exit.

Step III: Accept choice from user using INT 21H, function 01H.

Step IV: IS choice = 1 jump to step XI else goto step V.

Step V: IS choice = 2 jump to step XIV else goto step VI.

Step VI: IS choice = 3 jump to step XVII else goto step VII.

Step VII: IS choice = 4 jump to step XX else goto step VIII.

Step VIII: IS choice = 5 jump to step XXIII else goto step IX.

Step IX: Display Wrong choice.

Step X: Jump to step II.

Step XI: Call procedure accept.

Step XII: Accept string using INT 21H, function 0AH.

Step XIII: Return to main program and goto step II.

Step XIV: Call procedure length.

Step XV: Calculate the length of string and display it using INT 21H, function 02H.

Step XVI: Return back to main program and jump to step II.

Step XVII: Call procedure concatenate.

Step XVIII: Concatenate two strings and display.

Step XIX: Return back to main program and jump to step II.

Step XX: Call procedure compare.

Step XXI: Check if two strings are equal. If yes display strings are equal else strings are not equal.

Step XXII: Return back to main program and jump to step II.

Step XXIII: Terminate the program and stop.

**Concatenation of two strings**

**Program Statement:**

Write a program in the assembly language of 8086, to concatenate two strings.

**Explanation:**

Firstly, we will accept the two strings to be concatenated. Then, we will call procedure CONCAT which will concatenate the two strings. Display the concatenated strings.

**Algorithm:**

Step I: Start.

Step II: Accept string 1 from user.

Step III: Accept string 2 from user.

Step IV: Call procedure CONCAT.

Step V: Load length of string 1 in CX.

Step VI: Load the address of source string 1 in SI and DI.

Step VII: Copy the contents of string 1 to destination string.

Step VIII: Load SI with address of string 2.

Step IX: Copy the contents of string 2 to destination string.

Step X: Display the concatenated string.

Step XI: Procedure and return to calling program

Step XII: Stop

**Compare two strings**

**Program statement:**

Write a program in the ALP of 8086 to check the data in two strings are equal, if equal display the message “equal strings”, and if not display the message “unequal strings”.

**Explanation:**

We will accept two strings from the user. After accepting the strings, the first step in string comparison is to check whether their string lengths are equal. If the string lengths are not equal, we print the message unequal strings. If the string lengths are equal, we check if the contents of two strings are equal. The lengths of the two stings are initialized in the CX register.

The source and destination address are initialized in DS : SI and ES : DI registers.

Using the string instruction REPE CMPSB, two data are compared character by character.

If all the characters are matching display the message “equal strings” otherwise display “unequal strings”.

**Algorithm:**

Step I : Initialize the data memory.

Step II : Allocate data memory to save the strings.

Step III : Initialize DS and ES register.

Step IV : Accept the first string.

Step V : Accept the second string.

Step VI : Load the number of characters of first string in CL.

Step VII : Load the number of characters of second string in CH register.

Step VIII : Compare the lengths of the two strings. If not go to step XIII.

Step IX : Load number of characters to be compared in CX. Microprocessor & Interfacing Techniques (PU) L-24 Lab Manual

Step X : Compare the strings, character by character. If not same go to step XIII.

Step XI : Print “equal strings” using Macro.

Step XII : Jump to step XIV.

Step XIII : Print “unequal strings” using Macro.

Step XIV : Stop.

**Application:** Use of string operations in the Assembly Language programming to write modular program.

**Design:**

**Result and Discussion:**

.MODEL SMALL

.STACK

.DATA

M1 DB 10,13, "ENTER STRING 1: $"

M2 DB 10,13, "ENTER LENGTH OF STRING 1: $"

M3 DB 10,13, "DISPLAY STRING 1: $"

M4 DB 10,13, "ENTER STRING 2: $"

M5 DB 10,13, "ENTER LENGTH OF STRING 2: $"

M6 DB 10,13, "DISPLAY STRING 2: $"

M7 DB 10,13, "COMPARE STRINGS: $"

M8 DB 10,13, "STRING NOT EQUAL $"

M9 DB 10,13, "EQUAL STRING $"

M10 DB 10,13, "CONCATINATE STRINGS: $"

STR1 DB 50,?,50 DUP(?)

STR2 DB 50,?,50 DUP(?)

L1 DB ?

L2 DB ?

.CODE

DISP MACRO XX

MOV AH,09

LEA DX,XX

INT 21H

ENDM

.STARTUP

DISP M1 ;ENTER STRING 1

MOV AH,0AH ;Take Input of Whole string together

LEA DX,STR1

INT 21H

DISP M2 ;LENGTH OF THE STRING 1

LEA SI, STR1+1

MOV CL,[SI]

MOV L1,CL

ADD CL,30H

MOV DL,CL

MOV AH,02

INT 21H

DISP M3 ;DISPLAY STRING 1

LEA SI,STR1+2

MOV CL,L1

BACK1:

MOV DL,[SI]

MOV AH,02

INT 21H

INC SI

DEC CL

JNZ BACK1

DISP M4 ;ENTER STRING 2

MOV AH,0AH

LEA DX,STR2

INT 21H

DISP M5 ;LENGTH OF THE STRING 2

LEA DI, STR2+1

MOV CL,[DI]

MOV L2,CL

ADD CL,30H

MOV DL,CL

MOV AH,02

INT 21H

DISP M6 ;DISPLAY STRING 2

LEA DI,STR2+2

MOV CL,L2

BACK2:

MOV DL,[DI]

MOV AH,02

INT 21H

INC DI

DEC CL

JNZ BACK2

DISP M7 ;COMPARE STRINGS 1 & 2

MOV CL,L1

MOV CH,L2

CMP CL,CH

JNZ N\_EQUAL

LEA SI,STR1+2

LEA DI,STR2+2

BACK3:

MOV DL,[SI]

CMP DL,[DI]

JNZ N\_EQUAL

INC SI

INC DI

DEC CL

JNZ BACK3

DISP M9 ;CONCATE

JMP CONCATE

N\_EQUAL:

DISP M8

DISP M10

CONCATE:

MOV CL,L1

MOV BL,CL

MOV CH,L2

ADD BL,CH

LEA SI,STR1+2

LEA DI,STR2+2

BACK4:

INC SI

DEC CL

JNZ BACK4

BACK5:

MOV DL,[DI]

MOV [SI],DL

INC SI

INC DI

DEC CH

JNZ BACK5

LEA SI,STR1+2

BACK6:

MOV DL,[SI]

MOV AH,02

INT 21H


INC SI

DEC BL

JNZ BACK6

.EXIT

END

****

**Learning Outcomes:**

The student should have the ability to

LO1: List the string instructions

LO2: Describe the string addressing mode.

LO3: Use of string instructions in the program to perform different string operations.

**Course Outcomes**:

Upon completion of the course students will be able to make use of instructions of 8086 to build assembly and Mixed language programs.

**Conclusion:**

**Viva Questions:**

1. List the different string instructions.
2. Explain different string addressing modes.

**For Faculty Use**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Correction Parameters** | **Formative Assessment [40%]** | **Timely completion of Practical [ 40%]** | **Attendance / Learning Attitude [20%]** |  |
| **Marks Obtained** |  |  |  |